Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Disk Zone Status (`zoningcli` `list`)

If Hardware Management Pack software version 2.1.1 (or later) is installed on your system, you can use the `zoningcli` `list` command to determine whether or not zoning is enabled. Zoning status is shown in the first line of the output in each of the following examples.

Zoning is disabled:

    # zoningcli list expander
    Expander: SUN      SAS2 X16DBP      zoning: disable    <====
    ===================================================
    PHY  SAS ADDRESS    ZG   ZG Persist  att-dev att-id
    ===================================================
    00 5000c50017b0c149 010      1         01     00
    01 5000c5000576a349 010      1         01     00
    [...]
    25 0000000000000000 001      1         00     00
    ===================================================

Zoning is enabled:

    # zoningcli list expander
    Expander: SUN      SAS2 X16DBP      zoning: enable    <====
    ===================================================
    PHY  SAS ADDRESS    ZG   ZG Persist  att-dev att-id
    ===================================================
    00 5000c50017b0c149 010      1         01     00
    01 5000c5000576a349 010      1         01     00
    [...]
    25 0000000000000000 001      1         00     00
    ===================================================

If the `zoningcli` utility is not available on your system, you can use the OBP command `probe-scsi-all` to determine whether or not zoning is enabled. See Disk Zone Status (`probe-scsi-all`).

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |