Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

### Identifying WWN-Designated SAS2 Devices

These topics describe how to update the Oracle Solaris OS on Oracle’s SPARC T3 series servers.

- World Wide Name Syntax

- `probe-scsi-all` Output Example (SPARC T3-1, Eight-Disk Backplane)

- `probe-scsi-all` Output Example (SPARC T3-1, Sixteen-Disk Backplane)

- `probe-scsi-all` Output Example (SPARC T3-4)

- Identify a Disk Slot Using `probe-scsi-all` (OBP)

- Identify a Disk Slot Using `prtconf` (Oracle Solaris, Onboard Controllers)

- Identify a Disk Slot Using `prtconf` (Oracle Solaris, Single Initiator)

- WWN Syntax in an OS Installation on a Specific Device

- WWN Syntax in an OS Installation on a RAID Volume

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |