Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Operating Environment Requirements

Your environmental control system must provide intake air for the servers that complies with the limits specified inEnvironmental Specifications.

To avoid overheating, do not direct warmed air:

- Toward the front air intake of the server

- Toward the server access panels

Note - When you receive your server, place it in the environment where you will install it. Leave it in its shipping crate at its final destination for 24 hours. This resting period prevents thermal shock and condensation.

The servers have been tested to meet all functional requirements when operating in the operating environmental limits presented Environmental Specifications. Operating computer equipment in extremes of temperature or humidity increases the failure rate of hardware components. To minimize the chance of component failure, use the server within the optimal temperature and humidity ranges.

##### Related Information

- Airflow Considerations

- Minimum Clearance for Service Access

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |