Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Hard Drive Slot Configuration Reference

This topic describes the server's hard drive slot organization.

Address mapping between the Oracle Solaris OS device paths and physical hard drive slots is not fixed. For many storage administration tasks, the mapping of OS device names to physical hard drive slots must be determined before the task can be performed. See the SPARC T4 series servers administration guide for information on mapping SAS controller ports to physical drive slots.

Note - The server requires at least one hard drive to be installed and operational.

##### Eight-Drive Capable Backplane Configuration Reference

The following table identifies the drive slot numbering in an eight-drive capable backplane.

Table 28 Physical Drive Locations in an Eight-Drive Capable Backplane

HDD1 | HDD3 | HDD5 | DVD
HDD0 | HDD2 | HDD4 | HDD6 | HDD7

##### Sixteen-Drive Capable Backplane Configuration Reference

The following table identifies the hard drive slot numbering in a sixteen-disk capable backplane.

Table 29 Physical Drive Locations in a Sixteen-Disk Capable Backplane

HDD3 | HDD7 |  | HDD12 | HDD15
HDD2 | HDD6 |  | HDD11 | HDD14
HDD1 | HDD5 | HDD9 | DVD
HDD0 | HDD4 | HDD8 | HDD10 | HDD13

##### Related Information

- Hard Drive LEDs

- Remove a Hard Drive

- Install a Hard Drive

- Verify the Functionality of a Hard Drive

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |