Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a Power Supply

Note - This is a hot service procedure that can be performed by customers while the server is running. See Hot Service, Replaceable by Customer for more information about hot service procedures.

1. If the power supply bay contains a power supply filler panel, remove it.
2. Align the replacement power supply with the empty power supply chassis bay.
3. Slide the power supply into the chassis until it locks into place.
4. Plug the power cord into the power supply.

   Note - As soon as power is applied to the server, standby power initializes the SP. Depending on the server's OBP settings, the host server might automatically boot, or you might need to boot it manually.

5. Verify the functionality of the power supply.

   See Verify the Functionality of a Power Supply.

##### Related Information

- Remove a Power Supply

- Verify the Functionality of a Power Supply

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |