Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### PSH-Detected Fault Example

When a PSH fault is detected, an Oracle Solaris console message similar to the following example is displayed.

    SUNW-MSG-ID: SUN4V-8000-DX, TYPE: Fault, VER: 1, SEVERITY: Minor
    EVENT-TIME: Wed Jun 17 10:09:46 EDT 2009
    PLATFORM: SUNW,system_name, CSN: -, HOSTNAME: server48-37
    SOURCE: cpumem-diagnosis, REV: 1.5
    EVENT-ID: f92e9fbe-735e-c218-cf87-9e1720a28004
    DESC: The number of errors associated with this memory module has
    exceeded acceptable levels.  Refer to
    http://sun.com/msg/SUN4V-8000-DX for more information.
    AUTO-RESPONSE: Pages of memory associated with this memory module
    are being removed from service as errors are reported.
    IMPACT: Total system memory capacity will be reduced
    as pages are retired.
    REC-ACTION: Schedule a repair procedure to replace the affected
    memory module.  Use fmdump -v -u <EVENT_ID> to identify the module.

Note - The Service Required LED is also turned on for PSH-diagnosed faults.

##### Related Information

- PSH Overview

- Check for PSH-Detected Faults

- Clear PSH-Detected Faults

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |