Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Locate a Faulty Fan Module

This procedure describes how to identify the faulty fan using the Fan Fault LEDs.

| Caution - This procedure requires you to perform actions in an area that contains live voltages. Use caution to avoid contact with cable terminals or other electrified surfaces.

1. Check the front or rear panel System Fault LED.

   A fan fault will cause the System Fault LED (on front and rear of server) as well as a Fan Fault LED in the array of fan status LEDs to be lighted.

2. Extend the server to the maintenance position.

   See Extend the Server.

3. Release the two fan compartment door latches and swing the door open.
4. If the color of a Fan Fault LED is amber, replace the corresponding fan module.

   See Remove a Fan Module.

##### Related Information

- Fan Configuration Reference

- Fan Module LEDs

- Remove a Fan Module

- Install a Fan Module

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |