Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Oracle ILOM In-band (Sideband) Management

By default, you connect to the server’s SP using the out-of-band network management port (NET MGT). The Oracle ILOM sideband management feature enables you to select either the NET MGT port or one of the server’s Gigabit Ethernet ports (NETn), which are in-band ports, to send and receive Oracle ILOM commands to and from the server SP. In-band ports are also called sideband ports.

The advantage of using a sideband management port to manage the server’s SP is that one fewer cable connection and one fewer network switch port are needed. In configurations where numerous servers are being managed, such as data centers, sideband management can represent a significant savings in hardware and network utilization.

Note - In-band connection is not recommended for server modules.

When sideband management is enabled in Oracle ILOM, the following conditions might occur:

- Connectivity to the server SP might be lost when the SP management port configuration is changed while you are connected to the SP using a network connection, such as SSH, web, or Oracle ILOM Remote Console.

- In-chip connectivity between the SP and the host operating system might not be supported by the on-board host Gigabit Ethernet controller. If this condition occurs, use a different port or route to transmit traffic between the source and destination targets instead of using L2 bridging/switching.

- Server host power cycles might cause a brief interruption of network connectivity for server Gigabit Ethernet ports (NETn) that are configured for sideband management. If this condition occurs, configure the adjacent switch/bridge ports as host ports.

##### Related Information

- Configure SP In-band (Sideband) Access

- SP Network Address Options

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |