Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Insert and Lock the Server in the Rack

1. Insert the ends of the mounting brackets into the sliding rails.

   | Caution - The weight of the servers on extended slide rails can be enough to overturn an equipment rack.

   | Caution - The server weighs approximately 60 lb (25 kg). Two people are required to lift and mount the server into a rack enclosure when using the procedures in this chapter.

   | Caution - Before continuing, verify that the server is securely mounted in the rack, and that the slide rails are locked to the mounting brackets.

2. If the chassis or rack is equipped with an antitilt bar, deploy it.
3. Slide the chassis into the rack.

   Figure 23 Mounting the Chassis on the Slide Rails

##### Related Information

- Slide Rail Assembly Overview

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |