Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Platform-Specific Oracle ILOM Features

ILOM operates on many platforms, supporting features that are common to all platforms. Some ILOM features belong to only a subset of platforms. This topic describes the difference between ILOM features supported on the server and the common set of features described in the ILOM 3.0 base documentation.

Note - To perform some procedures documented in Oracle’s ILOM 3.0 base documentation, you must create a serial connection to the server and activate the Physical Presence switch on the server. For information about creating a serial connection, see the installation guide for your server.

Among the Oracle ILOM features supported on other platforms, Oracle ILOM does not support the following features on this server:

- Chassis monitoring module (CMM) features, such as single signon.

  Note - The T3 blade servers in a modular system do support the CMM features.

- POST diagnostics `user-reset` trigger is not available.

Oracle ILOM supports the following feature on this server, which may not be available on other platforms:

- POST diagnostics `hw-change` trigger. This new trigger (`hw-change error-reset`) is the default setting for the server, and causes POST to run each time the server is AC power-cycled, or the top cover is removed (if applicable). For more information on POST, see the service manual for your server.

##### Related Information

- Oracle ILOM Overview

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |