Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Input Power Overview

The SPARC T3-1 server can be equipped with one or two autoranging power supplies. They have the following input power requirements:

Specification | Values
--- | ---
System rating | 100Vac, 13A max, 50/60 Hz
| 110-127Vac, 12A max, 50/60 Hz
| 200-240Vac, 7A max, 50/60 Hz

To ensure redundant operation of the power supplies, connect the two power cords to separate circuits.

Tip - Do not connect the power supply cables before you connect a terminal device to the server. As soon as a power source is applied to the server, the service processor performs an initialization routine, which generatesmessages. If you do not have a terminal connected to the system before this starts, you will not see the initialization messages.

##### Related Information

- Server Specifications

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |