Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### LEDs for the Ethernet Ports and NET MGT Port

The following table describes the status LEDs assigned to each Ethernet port.

Table 21 Ethernet LEDs (NET0, NET1, NET2, NET3)

LED | Color | Description
--- | --- | ---
Left LED | Amber/Green | Speed indicator: Amber on – The link is operating as a 100-Mbps connection. Green on – The link is operating as a Gigabit connection (1000 Mbps). Off – The link is operating as a 10-Mbps connection.
Right LED | Green | Link/Activity indicator: Blinking – A link is established. Off – No link is established.

The following table describes the status LEDs assigned to the Network Management port.

Table 22 NET MGT Port LEDs

LED | Color | Description
--- | --- | ---
Left LED | Green | Link/Activity indicator: On or blinking – A link is established. Off – No link is established.
Right LED | Green | Speed indicator: On or blinking – The link is operating as a 100-Mbps connection. Off – The link is operating as a 10-Mbps connection.

##### Related Information

- Front Panel System Controls and LEDs

- Rear Panel System LEDs

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |