Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Guidelines for Planning Power Requirements

Use the following specifications only as a planning guide. For more precise power values, make power measurements on your specific server configuration using your planned workload. Refer to one of the following tables based on the model of your server.

Table 4 SPARC T3-1 Server (8-Disk Capacity) Power Specifications

General Specifications | Values
Operating input voltage range (input voltage tolerance +/- 10%) | 100 to 240 VAC, 50-60 Hz
Maximum operating input current at 100 VAC Maximum operating input current at 200 VAC | 8.4 A 4.2 A
Maximum operating input power at 100 VAC Maximum operating input power at 200 VAC | 800 W 792 W
Maximum heat dissipation | 2730 BTU/hour (2880 KJ/hour) 2702 BTU/hour (2851 KJ/hour)
Maximum standby power | 30 W
Inrush current (peak) | 25 A
Leakage current | 1.6 mA
Maximum Server Configuration Specifications Under Nominal Temperature and Voltage Conditions (16 core, 1.6 GHz processor, with sixteen 8 GB DIMMs, 8 HDDs, 6 PCIe I/O cards)
Idle input power | 416 W
Peak input power running SpecJBB | 582 W
Minimum Server Configuration Specifications Under Nominal Temperature and Voltage Conditions (16 core, 1.6 GHz processor, with four 2 GB DIMMs, 1 HDD, no PCIe I/O cards)
Idle input power | 290 W
Peak input power running SpecJBB | 352 W

Table 5 SPARC T3-1 Server (16-Disk Capacity) Power Specifications

General Specifications | Values
Operating input voltage range (input voltage tolerance +/- 10%) | 100 to 240 VAC, 50-60 Hz
Maximum operating input current at 100 VAC Maximum operating input current at 200 VAC | 9.4 A 4.7 A
Maximum operating input power at 100 VAC Maximum operating input power at 200 VAC | 896 W 888 W
Maximum heat dissipation at 100 VAC Maximum heat dissipation at 200 VAC | 3057 BTU/hour (3226 KJ/hour) 3030 BTU/hour (3197 KJ/hour)
Maximum standby power | 30 W
Inrush current (peak) | 25 A
Leakage current | 1.6 mA
Maximum Server Configuration Specifications Under Nominal Temperature and Voltage Conditions (16 core, 1.6 GHz processor, with sixteen 8 GB DIMMs, 16 HDDs, 6 PCIe I/O cards)
Idle input power | 494 W
Peak input power running SpecJBB | 678 W
Minimum Server Configuration Specifications Under Nominal Temperature and Voltage Conditions (16 core, 1.6 GHz processor, with four 2 GB DIMMs, 1 HDD, no PCIe I/O cards)
Idle input power | 297 W
Peak input power running SpecJBB | 359 W

Notes:

- The maximum operating input = {Max op input power} / Vac / 0.95 (for PSU PFC)

- W (AC) = W (DC) / 0.90 (for PSU efficiency)

- HDD power: 10W (DC) while busy (budgeted), 8W idle

- PCIe card pwer: 17W (DC) while busy (budgeted), 5W (DC) idle

##### Related Information

- Server Specifications

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |