Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Connect the NET MGT Port Cable

Before You Begin

The service processor network management port is labeled NET MGT. This port is located just to the right of the serial management (SER MGT) port on the rear panel.

- Connect a Category 5 cable from the NET MGT network management port to your network switch or hub.

  Figure 31 Service Processor Network Management Port – Rear Panel

  Note - This port is not operational until you configure the network settings (through the serial management port).

  Note - The service processor network management port is configured by default to retrieve network settings with Dynamic Host Configuration Protocol (DHCP) and allow connections using Solaris Secure Shell (SSH). You might need to modify these settings for your network. Instructions are given in Powering On the Server For the First Time.

##### Related Information

- Connect the SER MGT Port Cable

- Connecting the Server Cables

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |