Skip Navigation Links
Exit Print View
| SPARC T3-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Locate a Faulty DIMM Using the Remind Button

Use the DIMM Remind button to identify faulty DIMMs.

1. Extend the server to the maintenance position.

   See Extend the Server.

2. Disconnect power from the server.

   See Removing Power From the System.

3. Attach an antistatic wrist strap.
4. Remove the top cover.

   See Remove the Top Cover.

5. Swing the air duct up and forward to the fully open position.
6. Press the DIMM Remind button on the motherboard (callout 1 in the figure).

   This will cause an amber LED associated with the faulty DIMM to light for a few minutes.

7. Note the DIMM next to the illuminated LED.

   Figure Legend
   1 | Individual DIMM fault LEDs

8. Ensure that all other DIMMs are seated correctly in their slots.

##### Related Information

- Identify Faulty DIMMs Using the `show faulty` Command

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |