Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Specify the Hello Messaging Interval

This example transmits hello messages from `VLAN 5` to neighboring PIM routers every 80 seconds.

1. Enable PIM globally.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable

2. Enter Interface Configuration mode for the interface.

       SEFOS(config)# interface vlan 5

3. Associate the VLAN interface with the PIM component.

       SEFOS(config-if)# ip pim componentId 1

4. Configure the query interval for the PIM interface.

       SEFOS(config-if)# ip pim query-interval 80
       SEFOS(config-if)# end

5. Ensure that the correct PIM query interval is set.

       SEFOS# show ip pim interface detail
       Vlan5 33 is up
        Internet Address is 10.1.0.1
       Muticast Switching : Enabled
       PIM : Enabled
       PIMv6 : Disabled
       PIM version : 2, mode: Sparse
       PIM DR : 10.1.0.1
       PIM DR Priority : 1
       PIM Neighbour Count : 0
       PIM Hello/Query Interval : 80
       PIM Message Interval : 60
       PIM Override Interval : 0
       PIM Lan Delay : 0
       PIM Lan-Prune-Delay : Disabled
       PIM Component Id : 1
       PIM domain border : disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |