Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LAN Prune Delay

When you configure the PIMv6 LAN prune delay, you specify whether or not to use LAN prune delay.

1. Associate the `VLAN 7` interface with the PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. Enable the LAN prune-delay status for the `VLAN 7` interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# set ipv6 pim lan-prune-delay enable
       SEFOS(config-if)# end

3. Review the LAN prune-delay status.

       SEFOS# show ipv6 pim interface detail

       vlan7 34 is up
       ...
           PIM Lan-Prune-Delay: Enabled
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |