Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

#### Redistribution Overview

Redistribution is enabled by default when RIPng is enabled. You can disable or change redistribution status, allowing more control of distributing IPv6 routes. Available options are static, connected and OSPF routes, and metrics. The following example shows a configuration with the default redistribution values.

    SEFOS 1 SEFOS# show ipv6 rip
    RIP  port 521, multicast-group ff02::9,Maximum paths is 16
    Updates every 30 seconds; expire after 180
    Garbage Collect after  120 seconds
    Poison Reverse is on
    Interface:
    vlan40
    vlan10
    Redistribution:
     Connected, Routes Redistribution is enabled.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |