Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Network Type

The OSPF network type can be broadcast, nonbroadcast, point-to-multipoint, or point-to-point. The default type is broadcast. The OSPF network type can be configured to a type other than the default for a given media.

1. Configure the `VLAN 1` network type as point-to-point.

       SEFOS(config-if)# ip ospf network point-to-point

2. Examine the configuration information.

       SEFOS# show ip ospf interface vlan 1

       vlan1 is line protocol is up
       Internet Address 10.4.0.1, Mask 255.255.0.0, Area 0.0.0.0
       AS 1, Router ID 10.10.2.1, Network Type PointToPoint, Cost 1
       Transmit Delay is 1 sec, State 4, Priority 1
       Designated RouterId 10.10.2.1, Interface address 10.4.0.1
       No backup designated router on this network
       Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
       Hello due in 4 sec
       Neighbor Count is 0, Adjacent neighbor count is 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |