Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS5

In SEFOS5, area `0.0.0.4` is configured as a stub area.

- Type.

      SEFOS# configure terminal
      SEFOS(config)# router ospf
      SEFOS(config-router)# router-id 10.8.0.5
      SEFOS(config-router)# network 10.8.0.5 area 0.0.0.4
      SEFOS(config-router)# network 10.5.5.5 area 0.0.0.0
      SEFOS(config-router)# area 0.0.0.4 stub
      SEFOS(config-router)# exit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |