Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a Static Multicast Entry

To configure a static multicast entry for a specified VLAN, you must configure the VLAN prior to attempting to configure the static multicast entry. In addition, you must configure the member ports for that VLAN. In the following example, VLAN 2 is configured in the switch with member port 0/2 and a MAC address of `01:02:03:04:05:06`.

1. Configure static multicast entry in the VLAN table.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2
       SEFOS(config-vlan)# ports extreme-ethernet 0/2 untagged extreme-ethernet 0/2
       SEFOS(config-vlan)# exit

2. Configure the static multicast MAC address in the forwarding database.

       SEFOS(config)# mac-address-table static multicast 01:02:03:04:05:06 vlan 2 interface extreme-ethernet 0/2
       SEFOS(config)# exit

3. Review the configuration details.

       SEFOS# show mac-address table static multicast
       Static Multicast Table
       ----------------------
       VLAN            : 2
       Mac Address     : 01:02:03:04:05:06
       Receive Port    :
       Member Ports    : Ex0/2
       Forbidden Ports :
       Status          : Permanent
       Total Mac Addresses displayed: 1

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |