Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Acceptable Frame Type

You can configure the acceptable frame type for the port as one of the following:

- All frames

- Tagged frames

- Untagged and priority tagged frames

In the following example, the frame type is set to `tagged`.

1. Configure the acceptable frame type for the port.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/2
       SEFOS(config-if)# switchport acceptable-frame-type tagged
       SEFOS(config-if)# end
       SEFOS(config)# exit

2. Review the configuration information.

       SEFOS# show vlan port config port extreme-ethernet 0/2
       Vlan Port configuration table
       -------------------------------
       Port Ex0/2
       Port Vlan ID                        : 1
       Port Acceptable Frame Type          : Admit Only Vlan Tagged
       Port Ingress Filtering              : Disabled
       Port Mode                           : Hybrid
       Port Gvrp Status                    : Disabled
       Port Gmrp Status                    : Disabled
       Port Gvrp Failed Registrations      : 0
       Gvrp last pdu origin                : 00:00:00:00:00:00
       Port Restricted VLAN Registration   : Disabled
       Port Restricted Group Registration  : Disabled
       Mac Based Support                   : Disabled
       Subnet Based Support                : Disabled
       Port-and-Protocol Based Support     : Enabled
       Default Priority                    : 0
       Tunnel Status                       : Disabled
       Dot1x Protocol Tunnel Status        : Peer
       LACP Protocol Tunnel Status         : Peer
       Spanning Tree Tunnel Status         : Peer
       GVRP Protocol Tunnel Status         : Peer
       GMRP Protocol Tunnel Status         : Peer
       IGMP Protocol Tunnel Status         : Peer
       Filtering Utility Criteria          : Default
       Port Protected Status               : Disabled
       -------------------------------------------------------

   Note - When set to `tagged`, the device discards untagged and priority tagged frames received on the port. The device will process only the VLAN tagged frames.

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |