Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### SEFOS2 Configuration

See Sample Topology for setup information. In SEFOS2, VLAN interfaces `VLAN 5` and `VLAN 3` are configured as follows:

    SEFOS# configure terminal
    SEFOS(config)# set gvrp disable
    SEFOS(config)# set gmrp disable
    SEFOS(config)# interface vlan 5
    SEFOS(config-if)# shut
    SEFOS(config-if)# ip address 10.1.0.2 255.255.0.0
    SEFOS(config-if)# no shut
    SEFOS(config-if)# exit
    SEFOS(config)# vlan 5
    SEFOS(config-vlan)# ports extreme-ethernet 0/3 untagged extreme-ethernet 0/3
    SEFOS(config-vlan)# exit
    SEFOS(config)# interface vlan 3
    SEFOS(config-if)# shut
    SEFOS(config-if)# ip address 30.0.0.1 255.255.255.0
    SEFOS(config-if)# no shut
    SEFOS(config-if)# exit
    SEFOS(config)# vlan 3
    SEFOS(config-vlan)# ports extreme-ethernet 0/15 untagged extreme-ethernet 0/15
    SEFOS(config-vlan)# exit
    SEFOS(config)# interface extreme-ethernet 0/15
    SEFOS(config-if)# switchport pvid 3
    SEFOS(config-if)# no shut
    SEFOS(config-if)# exit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |