Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Port-Channel Interfaces

You can configure up to eight interfaces of the same type and speed for the same group. In the following procedure, port 0/3 on both switches is configured to be part of the LA. See LA Topology Example for the topology of this procedure. You must run all of the commands in the following procedure on both switches.

- Configure Port-Channel Interfaces

- Configure the LACP Port Priority

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |