Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Suppress Routing Updates on a Specified Interface

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf
       SEFOS(config-router)# router-id 10.10.2.1
       SEFOS(config-if)# passive-interface vlan 1

2. Examine the configuration details.

       SEFOS# show ip ospf interface vlan 1

       vlan1 is line protocol is up
       Internet Address 10.4.0.1, Mask 255.255.0.0, Area 0.0.0.0
       AS 1, Router ID 10.10.2.1, Network Type BROADCAST, Cost 1
       Transmit Delay is 1 sec, State 2, Priority 1
       No designated router on this network
       No backup designated router on this network
       Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
       No Hellos (Passive interface)
       Neighbor Count is 0, Adjacent neighbor count is 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |