Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Spanning Tree BPDU Transmit Status

If the BPDU transmit status on a port is disabled, no BPDUs are transmitted through that port.

- Specify the BPDU transmit status interface and configure the BPDU transmit status.

      SEFOS# configure terminal
      SEFOS(config)# interface extreme-ethernet 0/1

  Valid interfaces include physical interfaces and `port-channel` logical interfaces (`port-channel` port-channel-number).

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |