Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a Static Unicast Entry

To configure a static unicast entry, you must first configure the VLAN and the member ports for the specified VLAN. The following example shows port 0/2 on VLAN 2 being configured with the MAC address `22:22:22:22:22:22`.

1. Configure a static unicast entry in the VLAN table:.

       SEFOS# configure terminal
       SEFOS(config)# vlan 2

2. Configure a static VLAN entry with the required type of ports (0/2 in this example).

       SEFOS(config-vlan)# ports extreme-ethernet 0/2 untagged extreme-ethernet 0/2
       SEFOS(config-vlan)# exit

3. Configure a static unicast MAC address in the forwarding database.

       SEFOS(config)# mac-address-table static unicast 22:22:22:22:22:22 vlan 2 interface extreme-ethernet 0/2
       SEFOS(config)# end

4. Review the configuration details.

       SEFOS# show mac-address table static unicast
       Vlan  Mac Address        RecvPort Status   ConnectionId      Ports
       ----  -----------        -------- ------   ------------      -----
       2     22:22:22:22:22:22          Permanent                   Ex0/2

       Total Mac Addresses displayed: 1

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |