Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### L2 PVRST Configuration Task Overview

Use these tasks to configure L2 PVRST implementations of the topology. See L2 and L3 Topology.

Goal | Links
--- | ---
Configure standard L2 PVRST. | Configure Switch `ToR72p-1` for L2 PVRST Configure Switch `ToR72p-2` for L2 PVRST Configure Switch `ES1-24p-1` for L2 PVRST Configure Switch `ES1-24p-2` for L2 PVRST Verify the L2 PVRST Configuration
Configure L2 PVRST Active/Standby on the servers. | Prepare Switch `ToR72p-1` for L2 PVRST Active/Standby on the Servers Prepare Switch `ToR72p-2` for L2 PVRST Active/Standby on the Servers Configure Switch `ES1-24p-1` for L2 PVRST Active/Standby on the Servers Configure Switch `ES1-24p-2` for L2 PVRST Active/Standby on the Servers Verify the L2 PVRST Active/Standby Configuration on the Servers
Configure L2 PVRST LLA Active/Active on the servers. | Configure Switch `ES1-24p-1` for L2 PVRST LLA Active/Active on the Servers Configure Switch `ES1-24p-2` for L2 PVRST LLA Active/Active on the Servers Configure Switch `ToR72p-1` for L2 PVRST LLA Active/Active on the Servers Configure Switch `ToR72p-2` for L2 PVRST LLA Active/Active on the Servers Verify the L2 PVRST LLA Active/Active Configuration on the Servers

##### Related Information

- L2 and L3 Topology

- Configuring a Basic L2 PVRST Based Topology

- Configuring an L2 PVRST Based Topology With Active/Standby Bond on the Servers

- Configuring an L2 PVRST and LLA Based Topology With Active/Active Bond on the Servers

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |