Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Delete a Binding Entry From the Server

You can acquire an IP address dynamically for `vlan1` in switch 2.

1. View the binding table in switch 1.

       SEFOS# show ip dhcp server binding

       Ip         Hw              Hw           Binding      Expire
       Address    Type          Address        State        Time
       -------    -------        ------        --------     ----------
       12.0.0.2   Ethernet  00:02:02:03:04:01  Assigned     Jan  7 12:19:45 2007

2. Delete the binding entry for `12.0.0.2`.

       SEFOS# configure terminal
       SEFOS(config)# no ip dhcp binding 12.0.0.2
       SEFOS(config)# end

3. View the binding table in switch 1.

       SEFOS# show ip dhcp server binding
       SEFOS#

   Ensure that entry `12.0.0.2` is deleted and that the table is empty.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |