Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

## Display the Spanning Port Information

- Display the port information.

      SEFOS# show spanning-tree interface extreme-ethernet 0/1 detail
      Port 46 [Ex0/46] of MST00 is Root , ForwardingEx0/46 is operating in the MSTP ModePort path cost 2000, Port priority 128,Port Identifier 128.46. Port HelloTime 2,Timers: Hello - 0, Forward Delay - 0, Topology Change - 0Designated root has priority 32768, address 00:02:02:03:04:01Designated Bridge has priority 32768, address 00:02:02:03:04:01Designated Port Id is 128.46, Designated pathcost is 0Operational Forward delay 15, Max age 20Received Hello Time 2 SecNumber of Transitions to forwarding State : 2Auto-Edge is enabledPortFast is disabled, Oper-Edge is disabledLink type is point to PointBPDUs : sent 21, recieved 1331Restricted Role is disabled.Restricted TCN is disabled.bpdu-transmit enabledbpdu-receive enabledLoop Guard is disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |