Go to main content
oracle home
Sun Network 10GbE Switch 72p Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: November 2016

- Sun Network 10GbE Switch 72p Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Late-Breaking Information

- Switch Documentation Reading Order
- New Features

- IPv6 Switching and Routing
- PVRST+ Protocol
- Exclusive VLAN
- Data Center Bridging
- Internet Group Management Protocol
- PIM
- Q-in-Q Tunneling
- Server Load Balancer Layer 3
- Uplink Port Trailing
- VRRPv3
- Oracle ILOM 3.0 Features

- Enhancements
- Upgrading the Switch Firmware

- Back Up the Current Configuration Before Upgrading
- Download the Switch Firmware Package
- Install the Switch Updates

- Configuring the Switch

- Configure 1Gbps Mode on SFP+ Interfaces
- Fine Tune the VLAN Setup
- Managing SEFOS Configurations

- Include the SEFOS Configuration in Backups
- Restore the Configuration

- Configuring TACACS+

- TACACS+ Properties
- Configure TACACS+ Settings

- Known Issues

- Manually Deleting Static Routes Does Not Affect the Corresponding SLB Entry (7123134)
- PIMv6-SSM Mode is Not Supported in This Release (7114280)
- Firmware Upgrade With the Web UI is Incomplete (7022295)
- Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004)
- Some of the IGMP Conformance Results Do Not Match Expectations (7006297 and 6997415)
- QoS - set algo-type tailDrop queue-drop-algo Does Not Work (6991230)
- Packets Might Be Dropped When Using Q-in-Q Interop in Certain Configurations (6989048)
- The no default-metric [,short(1-16)>] Command Does Not Work as Documented (6987482)
- Using vlan 1 as Shown in Various Examples in the Documentation Generates Error Codes (6968484)
- When Multiple Configuration Scripts Are Run in Parallel, SEFOS Can Crash (6936742)
- The switch Command Line Option Is Unsupported
- vrrp_v3: Role is incorrect for vlan with no premempt configuration after save/reboot (19547263)
- SSL V3.0 POODLE DISABLE SSL V3 (19842635)
- Re-configure IP address after a "no ip address", previous config re-appears (18794861)

Language:

### TACACS+ Properties

CLI Property | Default Value | Description
--- | --- | ---
`address [tacacs+_server_IP_address]` | `0.0.0.0` | Specifies the IP address or DNS name of the TACACS+ server. If you use DNS, ensure that DNS is configured and functional.
`Defaultrole [a|u|o|c|r|s|Administrator|Operator]` | `Operator` | Specifies the access role that is granted to all authenticated TACACS+ users. This property supports the following legacy roles: `Administrator` `Operator` Any individual role ID combinations where a = Admin, u = User Management, o = Operator, c = Console, r = Reset and Host Control, and s = Service.
`fs_privilege` [1|15] | `1` | Specifies the fs_privilege that is used for TACACS+ authenticated users to access and control SEFOS.
`port [port_number]` | `49` | Specifies the port number used to communicate with the TACACS+ server.
`protocol` `service` | `ip` ppp | `protocol` identifies the TACACS+ protocol type. `service` identifies the TACACS+ service type. (see footnote) In the TACACS+ server, the combination of ppp and ip can be configured to send additional fields in packet data. For Oracle ILOM clients this is used to send Oracle ILOM-specific fields like sefos-fs-privilege and ilom-role.
`secret [tacacs+_secret]` | [none] | Specifies the shared secret that is used to protect sensitive data and to ensure that the client and server recognize each other.
`state [enabled|disabled]` | `Disabled` | Specifies whether the TACACS+ client is enabled or disabled.

Previous
Next