Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### NET MGT Port

Two RJ-45 network management ports are located on the front left of the switch. See Front Panel Components.

Use NET MGT 0 (Port A) to provide Ethernet CLI and web interface connections to a system console for administering the switch remotely.

The NET MGT connector is a 100 BASE-T Ethernet interface. This connector is preferred because it permits remote management of the switch over the Ethernet network.

Note - Do not use NET MGT 1 (Port B). Port B is functional but currently has some limitations and is not supported at this time.

This figure and table describe the pinouts of the NET MGT connector.

Pin. | Signal
--- | ---
1 | TXD+
2 | TXD-
3 | RXD+
4 | Not used
5 | Not used
6 | RXD-
7 | Not used
8 | Not used

##### Related Information

- SER MGT Port

- Management Cable Requirements

- Connect the NET MGT Cable

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |