Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Report Forward Suppression Interval

The default report forward interval is 5 seconds. This example sets the report-forward interval to 8 seconds. MLD report messages for the same group will not get forwarded onto the router ports for 8 seconds.

1. Configure the report-suppression interval.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 mld snooping report-suppression-interval 8
       SEFOS(config)# end

   Only one report will be forwarded within the report forward interval of 8 seconds for a particular group.

2. View the configuration.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
       -----------------------------
       MLD Snooping globally enabled
       MLD Snooping is operationally enabled
       Multicast forwarding mode is MAC based
       Proxy reporting globally enabled
       Router port purge interval is 125 seconds
       Port purge interval is 130 seconds
       Report forward interval is 8 seconds
       Group specific query interval is 2 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |