Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Debug Traces for the DHCP Server

1. Enable the debug trace for the DHCP server.

       SEFOS# debug ip dhcp server all

2. View the debug trace level.

       SEFOS# show ip dhcp server information

   The output in switch 1 is:

       DHCP server status                     : Enable
       Send Ping Packets                      : Disable
       Debug level                            : All
       Server Address Reuse Timeout           : 5 secs
       Next Server Address                    : 0.0.0.0
       Boot file name                         :

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |