Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the RP Static Address

Static configuration allows additional structuring of the multicast traffic by directing the multicast join or prune messages to statically configured RPs.

1. Associate the `VLAN 7` interface with the PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. Enable the static-RP configuration for the router.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim static-rp enable

3. Enter the PIMv6 component mode for the component (2 in this example).

       SEFOS(config)# ip pim component 2

4. Set the RP static RP address (`7777::11`) with a mask length of 128 for group `ff02::e001:1` in PIMv6 component 1.

   This step uses the following parameters:

   - RP address: `7777::11`

   - Mask length: `128`

   - Group address: `ff02::e001:1`

       SEFOS(pim-comp)# ipv6 pim rp-static rp-address ff02::e001:1 128 7777::11
       SEFOS(pim-comp)# end

5. Review the RP static RP address.

       SEFOS# show ipv6 pim rp-static 2

       Static-RP Enabled
       CompId    GroupAddress/PrefixLength       RPAddress
       ------    -------------------------       ---------
            2             ff02::e001:1/128           7777::11

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |