Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

### Verifying DCB and LLDP Configurations

If both peers that are connected to port 2 and port 18 have been configured properly, you can use various `show` commands to verify the configurations. Use the following commands to display the configurations and verify that a DCB feature is configured correctly, and that DCBX TLVs are exchanged with a peer.

- Determine VLAN Assignment

- Determine Whether Interfaces Are Active

- Determine Whether LLDP is Running and Recognizing Peers

- Enable DCB

- Disable DCB

- Enable DCB for Each Interface

- Disable DCB for Each Interface

- Enable and Disable a Specific DCB Feature

- Configure the Mode for the DCB Feature

- Configure DCB Attributes

- Configure LLDP DCBX TLVs

- Display DCBX Feature Statistics and Control Information

- Display Output of Unstarted DCBX Protocol Exchange

- Display Output of DCBX TLV Exchange

- Display Output of No TLV Exchange

- Clear Feature Statistics

- Display Output Showing a Down Link

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |