Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Acronyms and Abbreviations

Acronym or Abbreviation | Explanation
--- | ---
ABR | Area border router
AH | Authentication header
AS | Autonomous system
ASBR | Autonomous system border router
BGP | Border Gateway Protocol
CLI | Command-line interface
DDP | Database description packet
DR | Designated router
ESP | Encapsulating security payload
IPsec | IP Security Protocol
IPv6 | Internet Protocol version 6
ISM | Interface state machine
LAN | Local area network
LSA | Link state acknowledgment packet
LRQ | Link state request packet
LS | Link state
LSA | Link state advertisement
LSDB | Link state database
LSP | Label-switched path
LSU | Link state update
NBMA | Non-broadcast multi-access
ND | Neighbor discovery
NSSA | Not-so-stubby-area
OSPFv3 | Open Shortest Path First version 3
RIP | Routing Information Protocol
RRD | Route redistribution
RTM6 | Route table manager for IP version 6
SEFOS | Sun Ethernet Fabric Operating System
SPF | Shortest Path First
VLAN | Virtual LAN
VPN | Virtual private network
VRF | Virtual routing and forwarding

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |