Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Reset the DAD Attempts

1. Enter Interface Configuration mode for the `VLAN 1` interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Reset the number of DAD attempts.

       SEFOS(config-if)# no ipv6 nd dad attempts

3. Review the DAD attempts in the `VLAN 1` interface information.

       SEFOS# show ipv6 interface vlan 1

       vlan1 is up, line protocol is up
       ...
           ND DAD is enabled, Number of DAD attempts: 0
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |