Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Create a PIMv6 Neighbor

Before you attempt to use the instructions in this section, you must enable PIMv6 in router A and router B so that they exchange the PIMv6 hello message and form neighbors. See Enable PIMv6 for instructions.

1. In both routers, associate the `VLAN 7` interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. In router A, review the PIMv6 neighbor router for the PIMv6 enabled router.

       SEFOS# show ipv6 pim neighbor

       Neighbor IfName/Idx Uptime/Expiry Ver   DRPri CompId  Override   LanDelay
       Address                                  /Mode          Interval
       --------- ---------- ------------- ---    -----   ------   -------    -------
       fe80::7777::21 vlan7/34   00:02:09/95    v2  1         1         0   0

3. In router A, review the PIMv6 neighbor for `VLAN 7`.

       SEFOS# show ipv6 pim neighbor vlan 7

       Neighbor    IfName/Idx Uptime/Expiry Ver DRPri   CompId   Override  LanDelay
       Address                                  /Mode            Interval

       ---------      ---------- ------------- --- -----   ------   --------  --------
       fe80::7777::21 vlan7/34   00:09:30/75    v2  1         1         0   0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |