Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

This table contains the default values assigned to the IPv6 features during the startup of the switch. These values are referenced throughout this guide.

Feature | Default Setting
--- | ---
IPv6 on an interface | DisabledEnabled on the default VLAN interface
Unicast routing | Enabled
Default prefix | Unicast
Route administrative distance | 1
Router advertisement status | Disabled (suppressed)
Hop limit | 64
RA lifetime | 1800 seconds
Number of duplicate address detection attempts | 1
ND reachable-time | 30 seconds
RA interval | 600 seconds
RA valid lifetime | 25,9200 seconds
RA preferred lifetime | 60,4800 seconds
Data to be sent in the `ping`(1) message | a5a5
`ping`(1) messages repeat count | 5
Size of the `ping`(1) message | 100 bytes
`ping`(1) timeout value | 5 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |