Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Completing Preliminary Configurations

You can configure SEFOS IPv6 features by accessing Global Configuration mode or Interface Configuration mode. The configuration steps in this document begin with accessing one or both of these modes. See the CLI Command Modes. These procedures are part of the preliminary configurations that you must execute before you can configure the IPv6 features.

- Create an Interface

- Configure an IPv4 Address for an Interface

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |