Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Proxy Reporting

By default, proxy reporting is enabled. If you have previously disabled the feature, you can re-enable it.

1. Configure proxy reporting.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 mld snooping proxy-reporting

2. View the configuration.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
       -----------------------------
       MLD Snooping globally disabled
       MLD Snooping is operationally disabled
       Multicast forwarding mode is MAC based
       Proxy reporting globally enabled
       Router port purge interval is 125 seconds
       Port purge interval is 260 seconds
       Report forward interval is 5 seconds
       Group specific query interval is 2 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |