Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Set the DAD Attempts

1. Enter Interface Configuration mode for the `VLAN 1` interface

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1

2. Set the number of DAD attempts.

       SEFOS# ipv6 nd dad attempts 5
       SEFOS(config)# exit

3. Review the DAD attempts in the `VLAN 1` interface information.

       SEFOS# show ipv6 interface vlan 1
       vlan1 is up, line protocol is up
       ...
       ND DAD is enabled, Number of DAD attempts: 5
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |