Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable Query Transmission on Topology Change

If you have enabled the transmission of MLD queries when topology changes occur in the network, you can disable the feature.

1. Restore the default value of the query transmission on topology change feature.

       SEFOS(config)# ipv6 mld snooping send-query disable

2. Ensure that queries will not be transmitted when a topology change occurs.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
         -----------------------------
         MLD Snooping globally enabled
         MLD Snooping is operationally enabled
         Transmit Query on Topology Change globally disabled
         Multicast forwarding mode is MAC based
         Proxy reporting globally enabled
         Router port purge interval is 125 seconds
         Port purge interval is 260 seconds
         Report forward interval is 5 seconds
         Group specific query interval is 2 seconds
         Reports are forwarded on router ports
         Group specific query retry count is 2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |