Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

## Restart the Server Following Failure

When the failed server is repaired and restored (starts responding to ICMP ping from the switch again), it resumes in the active state, and the failover server resumes in standby state. This situation is demonstrated in this example by bringing the ixgbe0 network interface on server 1 backup.

- Type.

      server1% ifconfig ixgbe0 up
      SEFOS# show slb

      SLB Group ID: 1 Virtual IP: 10.10.10.0/24
      Server Members:
      IP Address       Vlan  MacAddress        Port State     Comments
      ================ ====  ================= ==== ========= ==================
      192.0.0.1        3     00:1b:21:53:6e:e0    9 ACTIVE
      192.0.0.2        3     00:1b:21:53:6f:00    9 ACTIVE
      192.0.0.3        3     00:3e:16:20:12:01    9 ACTIVE
      192.0.0.4        3     00:3e:15:18:05:30    9 STANDBY   (up)

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |