Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

#### Sensors Overview

The switch uses several configurable sensors and indicators to monitor switch power, voltage, and temperature. The switch includes replaceable component sensors that generate entries in the SEL when the sensor crosses a threshold. Many of these readings are used to adjust the fan speeds and perform other actions, such as illuminating LEDs and powering off the switch.

You can also configure these sensors to generate IPMI PET and SNMP traps, as described in the Sun Integrated Lights Out Manager (ILOM) CLI Procedures Guide.

| Caution - Do not use any interface other than the Oracle ILOM CLI or web interface to alter the state or configuration of any sensor or LED. Doing so could void your warranty.

You can view the system monitoring sensors and indicator parameters from the Oracle ILOM CLI or web interface.

- Sensors Overview

- Identifying LEDs

##### Related Information

- Sun Integrated Lights Out Manager (ILOM) Concepts Guide

- Sun Integrated Lights Out Manager (ILOM) 3.0 Management Protocols Reference Guide

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |