Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

## Determine VLAN Assignment

- Type the `show vlan id` command to determine VLAN assignment.

  In the sample configuration, port 2 and port 18 must have `VLAN 201` assigned to them.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |