Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Neighbor Probe Retransmission Limit

This example specifies that the neighbor will be deemed inactive after 20 consecutive LSA transmissions.

1. Configure the number of consecutive LSA retransmissions before the neighbor is deemed inactive.

       SEFOS(config)# interface vlan 10
       SEFOS(config-if)# ipv6 ospf demand-circuit
       SEFOS(config-if)# ipv6 ospf neighbor-probe retransmit-limit 20
       SEFOS(config-if)# end

2. Ensure that the correct retransmission limit was set.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information

       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: BROADCAST     Cost: 1             State: BACKUP
       Designated Router Id: 10.0.0.8      local address: fe80::214:4fff:fe6c:d04d
       Backup Designated Router Id: 10.0.0.1      local address: fe80::214:4fff:fe6c:628f
       Transmit Delay: 1 sec        Priority: 1         IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Enable             Neighbor Probing: Enable
       Nbr Probe Retrans Limit: 20        Nbr Probe Interval: 120
       Hello due in 5 sec
       Neighbor Count is: 1
       Adjacent with neighbor 10.0.0.8

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |