Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### Oracle Switch ES1-24

Oracle Switch ES1-24 is a standalone half-width 1U, 10GbE switch. The switch provides 20 10GBASE-T ports supporting 100M/1G/10GbE and four SFP+ ports supporting 1/10GbE. The switch rackmount kit supports either single or dual switch configurations.

For installation, configuration, and management information, refer to the documentation at: http://www.oracle.com/goto/ES1-24/docs

##### Additional L2 and L3 Configurations for Oracle Switch ES1-24

For the following configurations, refer to the Oracle Switch ES1-24 Configuration Guide at: http://www.oracle.com/goto/ES1-24/docs

- Switching Feature

  - VLAN Forwarding

  - RSTP

  - LA

- Routing Feature

  - Static Unicast Route Entries

  - Dynamic Routing with RIP

  - Dynamic Routing with OSPF

##### Related Information

- Sun Network 10GbE Switch 72p

- Sun Blade 6000 Ethernet Switched NEM 24p 10GbE

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |