Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Snooping Query Interval

The IGS query interval refers to the time interval during which the switch waits after sending a group-specific query to determine if hosts are still interested in a specific multicast group.

1. Enter the configure mode for the VLAN.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4

2. Configure the query interval.

       SEFOS(config-vlan)# ip igmp snooping query-interval 60
       SEFOS(config)# end

3. Review the configuration.

       SEFOS# show ip igmp snooping

       Snooping VLAN Configuration for the VLAN 4
         IGMP Snooping enabled
         IGMP configured version is V3
         Fast leave is disabled
         Snooping switch is configured as Querier
         Snooping switch is acting as Querier
         Query interval is 60 seconds
         Port Purge Interval is 130 seconds
         Max Response Code is 100, Time is 10 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |